## Section 569. — CONCRETE OVERLAYS FOR BRIDGE DECKS

07/20/15–FP14

WFL Specification 07/20/15 5690010

Use the following when work is required in this Section.

Construction Requirements

### 569.04 Composition (Concrete Mix Design).

Amend as follows:

Delete item **(b)** in the first paragraph and substitute the following:

**(b)** Section 4 of ACI 301, *Specifications for Structural Concrete,* for determining required average compressive strength (f’cr).

Delete the first sentence of the third paragraph and substitute the following:

Verify mix designs with trial mixes prepared according to ACI 301 from proposed sources or with previous concrete production data for the mixture design submitted from proposed sources.